KX-6000 系列 UOS 64bit Driver Release Note

2025-7-4

Support Platforms

Display Support

Change History

Installing and uninstalling driver

Support Platforms

Support CHIPS:

KX-6000 系列 Chip

Support OS:

UOS_64bit

Support LINUX

Linux Kernel 4.19/5.10/6.6

Driver Version:

zhaoxin-linux-graphics-driver-dri-21.00.77_amd64.deb

Back to top

Display Support

Support Device:

CRT , DP1/HDMI1/DVI1, DP2/HDMI2/DVI2

Resolution Support

Note: DRAM with 1&4 slot and 2&3 slot are snoop only cases, others can support none snoop

a) FB size = 64MB, support single view only

Device Combination | Max Resolution
Integrated DisplayPort1/DisplayPort2 | 1920x1080@60Hz
Integrated CRT | 1920x1080@60Hz
Integrated HDMI1/HDMI2 | 1920x1080@60Hz
Integrated DVI (through Integrated HDMI1/HDMI2) | 1920x1080@60Hz

b) FB>64MB and Snoop only, can support multi view

Max Resolution is 1920x1080@60Hz.

c) FB>64MB and none snoop , can support multi view

输出设备 1 | 输出设备 2 | 输出设备 3 | 输出设备 1 最大分辨率 | 输出设备 2 最大分辨率 | 输出设备 3 最大分辨率
CRT | \ | \ | 2048x1536@60Hz | \ | \
DVI | \ | \ | 1920x1200@60Hz | \ | \
HDMI\DP\eDP | \ | \ | 4096x2160@60Hz | \ | \
CRT | DVI | DVI | 2048x1536@60Hz | 1920x1080@60Hz | 1920x1080@60Hz
CRT | HDMI\DP\eDP | HDMI\DP\eDP | 1920x1080@60Hz | 4096x2160@60Hz | 1920x1080@60Hz

a) 多设备输出包含复制和扩展两种模式; WinXP 单屏最大分辨率为 2048x1536@60Hz

b) 4K 显示分辨率下用户体验较差,且性能体现较大依赖于应用场景和应用程序.受限于 GPU 性能,任意显示设备启用 4K 显示分辨率后,不论何种显示组合均会受到此影响.

Open API Support

1. GLX1.4

2. OpenGL3.2

3. EGL1.4

4. OpenGL ES2.0

Video Codec Support

1. Decoding Capabilities

Format | Performance | Profile
H.265 HEVC | 1920x1080p30@100Mbps 1920x1080p120@25Mbps 4096x2160p30@100Mbps | MP
H.264 AVC | 1920x1080p30@70Mbps 1920x1080p120@25Mbps 3840x2160p30@50Mbps | HP
VP8 | 1920x1080p30@10Mbps | /
M-JPEG | 1920x1080p30@80Mbps (M-JPEG) Baseline 8kx4k, 130Mpps (JPEG) | Baseline
VC-1/WMV9 | 1920x1080p30@72Mbps | Level:AP@L3.0
AVS | 6.0.3.08.60(base),1920x1152p60@65Mbps 6.0.0.08.60(broadcast),1920x1152p60@25Mbps | /

Note:

a) UOS 系统自带的深度影院可以支持硬解。

b) 21.00.30 版驱动(包括)之后的驱动支持 HEVC 和 H264 最大解码宽高放开为 4096x2304

2. Video Capabilities

a) 1080i@60/50Fps clips can not be supported in 4k@30Hz mode.

b) no moving window, no resizing window with one single 4k@30fps video

c) some media player may have different behavior and it may have some background 3D BLT even it is in full screen mode.

3. Encoding Capabilities

Format | Performance | Profile
H.265 HEVC | 1920x1080p@60fps | MP/I, P frames/CABAC
H.264 AVC | 1920x1080p@60fps | HP/I, P frames/CAVLC

Test Note:

1. Test with C-state disabled as it will affect performance.

Disable c-state in BIOS setup

a) Power on and press “F2” on keyboard

b) In Advanced — CPU configuration — Chipset Cx State Configuration

c) CPU Processor C state to “Disable”

d) At last press “F10” to save & Exit.

2. 系统跑 Benchmark 分数之前需要关闭 Vsync，关闭 Vsync 的命令如下： #export VBLANK_MODE=0

3. HDMI 插拔，有概率遇到拔出 HDMI 接口后状态不变，这跟插拔手法，速度，接口硬件等因素有关， 遇到问题的根本原因是如果中断信号先触发，但是 EDID 信号还没断开，驱动仍然检测到显示器，就 不会向 OS 报告 hotplug event。通过更换 HDMI cable 或者调整插拔手法，确保中断信号和 EDID 信 号同时断开可以避免该问题的发生。

4. 21.00.57（包含）开始，可以支持对全部旧驱动的覆盖安装。21.00.57 之前的驱动覆盖安装功能不完善.

5. Mesa23 不支持原来的 dri driver，需要重新适配 glvnd driver。驱动会检查系统的 mesa 版本，mesa23 及以上版本的系统需要安装 glvnd driver，原来的 dri driver 会继续支持旧版本系统。

Back to top

Change History

21.00.77（2025/7/4）

Bug Fix:

1. DP 显示优化。

21.00.75（2025/4/24）

Bug Fix:

1. 信创端观看安卓端视频流时，会出现小视频画面花屏现象

21.00.74（2025/3/28）

Bug Fix:

1. 客户 reboot 压测概率 eDP 显示花屏

21.00.73（2025/2/26）

Bug Fix:

1. https://sketchfab.com/3d-models/lamborghini-huracan-twin-turbo-lost-1d3809 ea5a6749d9864ec4c32511d716 无法正常渲染问题

2. https://robostorm.io/无法正常渲染问题

3. 欧灵屏设计缺陷导致 HPD 异常拉低的问题，需要 driver patch

4. Edp Panel 4K@60hz 屏幕闪烁问题

21.00.72（2025/1/20）

Bug Fix:

1. 修复客户软件应用不定时花屏问题。

2. 客户 HDMI CTS 认证 fail 问题

21.00.71（2024/12/13）

Bug Fix:

1. 修复客户平台，UOS1070 播放 4K 视频花屏问题。

21.00.70（2024/11/5）

New Feature/Update：

支持在 BIOS 里增加 flag，用来区分主板是否接 re-timer

21.00.69(10/8/2024)

Bug Fixed:

1. KX-U6780A 基于 UOS1060 一体机亮度调节

2. 改善 SI 的 Linux 驱动需求

3. UOS1060 中控不显示问题

4. <统信>UOS1060 通用版运行 scratch3 报错问题

5. UOS1070 百度网盘播放适配黑屏问题

21.00.68（9/4/2024）

Bug Fixed

1. <统信>UOS 1071 系统登录密码输入错误 4 次，弹出密码重置提示，点击重置密码后无法调出重置框

2. UOS 浏览器访问网页 https://webglfundamentals.org/，几分钟后导致物理内存就会跑满系统卡死

3. 希沃白板立体几何渲染异常

21.00.67（8/14/2024）

Bug Fix:

1. 客户笔记本 UOS 打开 vmware 客户端，系统自动注销问题

2. KX-U6780A+UOS 平台，h264_vaapi 编码器初始化失败问题

21.00.66（8/7/2024）

Bug Fix:

1. 修改 KX-U6980S HDMI 最大分辨率为 2560x1440@30Hz，DP 最大分辨率为 3840x2160@30Hz，DP 默认 SSC disable，通过 BIOS Setting 来配置

21.00.65（7/11/2024）

Bug Fix：

1. 客户问题 KVM switch 接 VGA，集显启动过程不插显示器到启动后再插上会不显示画面

2. 客户会议 APP 加入会议后花屏

3. 统信 dkms 包中的 dkms.conf 文件添加 config：SKIP_IMMD_MODPROBE=1

21.00.63（4/1/2024）

Bug Fix：

客户问题<Video>VLC 循环播放视频后，拔掉 HDMI 一分钟后插上终端报错

21.00.62（3/21/2024）

New Feature：

驱动支持 mesa23 同时可以向下兼容较低 mesa 版本

Bug Fix：

EDP 重启闪屏问题

21.00.61（1/26/2024）

1. 全功能 TYPE-C 4K 60HZ 黑屏

Back to top

Installing and uninstalling driver

i. Install driver

#dpkg -i zhaoxin-linux-graphics-driver-dri-21.00.XX_amd64.deb

Input command #reboot to restart the system.

Checking whether the driver is installed successfully

Open terminal and input command #dpkg -l | grep zhaoxin

Note: the name and version of the driver will show: ii zhaoxin-linux-graphics-driver-dri:amd64 21.00.XX

ii. Uninstall driver

1. 查看系统的驱动：

#dpkg -l | grep zhaoxin

2. 会打印出driver 信息: ii zhaoxin-linux-graphics-driver-dri:amd64 21.00.xx.

3. 卸载驱动

#dpkg -P zhaoxin-linux-graphics-driver-dri:amd64用步骤1中看到的驱动名字

4. 重启系统

#reboot

Back to top