KX-6000 Win11 64bit Universal Driver Release Note

2022-07-14

Support Platforms

Display Support

Installing and uninstalling driver

Revision History

Support Platforms

Support CHIPS:

KX-6000 Chip

Support OS:

Win11 64bit-21H2(OS Build 22000.194)

Driver Version:

10.17.19.00.34-37.00.34

Back to top

Display Support

Support Device:

CRT , DP1/HDMI1/DVI1, DP2/HDMI2/DVI2

Resolution Support

Note: DRAM with 1&4 slot and 2&3 slot are snoop only cases, others can support none snoop

a) FB size = 64MB, support single view only

Device Combination | Max Resolution
Integrated DisplayPort1/DisplayPort2 | 1920x1080@60Hz
Integrated CRT | 1920x1080@60Hz
Integrated HDMI1/HDMI2 | 1920x1080@60Hz
Integrated DVI (through Integrated HDMI1/HDMI2) | 1920x1080@60Hz

b) FB>64MB and Snoop only, can support multi view

Max Resolution is 1920x1080@60Hz.

c) FB>64MB and none snoop , can support multi view

输出设备 1 | 输出设备 2 | 输出设备 3 | 输出设备 1 最大分辨率 | 输出设备 2 最大分辨率 | 输出设备 3 最大分辨率
CRT | \ | \ | 2048x1536@60Hz | \ | \
DVI | \ | \ | 1920x1200@60Hz | \ | \
HDMI\DP\eDP | \ | \ | 3840x2160@60Hz | \ | \
CRT | DVI | DVI | 2048x1536@60Hz | 1920x1080@60Hz | 1920x1080@60Hz
CRT | HDMI\DP\eDP | HDMI\DP\eDP | 1920x1080@60Hz | 3840x2160@60Hz | 1920x1080@60Hz

Open API Support

1. OGL 3.2

2. OCL 1.1

DirectX API Support

1. DX 9.3

2. DX 10.1

3. DX 11.0

Video Codec Support

1. Decoding Capabilities

Format | Performance | Profile
H.265 HEVC | 1920x1080p30@100Mbps 1920x1080p120@25Mbps 4096x2160p30@100Mbps | MP
H.264 AVC | 1920x1080p30@70Mbps 1920x1080p120@25Mbps 3840x2160p30@50Mbps | HP
VP8 | 1920x1080p30@10Mbps | /
M-JPEG | 1920x1080p30@80Mbps (M-JPEG) Baseline 8kx4k, 130Mpps (JPEG) | Baseline
VC-1/WMV9 | 1920x1080p30@72Mbps | Level:AP@L3.0
AVS | 6.0.3.08.60(base),1920x1152p60@65Mbps 6.0.0.08.60(broadcast),1920x1152p60@25Mbps | /

Note:

a) Win10 "Movie&TV" can support HEVC HW decoding need install filter "HEVC Video Extension"(https://www.microsoft.com/en us/store/p/hevc video extension/9n4wgh0z6vhq)

b) Win10 WMP only support H.264, VC-1 HW decoding.

c) Windows OS has no filter, cannot support AVS decode.

2. Video Capabilities

a) 1080i@60/50Fps clips can not be supported in 4k@30Hz mode.

b) No moving windows and no resizing windows with one single 4k video on 4k mode.

c) Some media player may have different behavior and it may have some background 3D BLT even it is in full screen mode.

3. Encoding Capabilities

Format | Performance | Profile
H.265 HEVC | 1920x1080p60 (Not WHQL Certified) | MP/I, P frames
H.264 AVC | 1920x1080p60 (WHQL Certified) | HP/I, P frames

Back to top

Installing and uninstalling driver

Note：Universal driver can be installed by Univesal_xxx64.inf file only, no setup.exe.

i. Manually installing the display driver package

1. Press Win+R buttons on your keyboard to open "Run..." dialog

2. Type "devmgmt.msc", and then click "OK" to open Device Manager

3. Click "Display adapters"--> Right click "Microsoft basic Display Adapter" --> Click"Update driver"

4. Click "Browse my computer for drivers software"

5. Click "Browse" to select the folder that contains drivers for ZX GPU, then click OK

6. Click Next to install Driver

7. Reboot your system after the "Windows has successfully updated your drivers" page pop up

ii. Uninstalling the software

1. In Device Manager, Right Click "ZX 960 GPU", Click "Uninstall device"

2. Check "Delete the driver software for this device",then click "uninstall" button to uninstall driver

3. Reboot your system after uninstallation finished

Back to top

Revision History

Version | Release Date | Comments
10.17.19.0034-37.00.34 | 2022-07-14 | ü Add 4part ID for customer ü Add 2part ID for Generic Package
10.17.19.0033-37.00.33 | 2021-10-29 | ü 适配 Win11 x64 B22000.194 ü Add 4part ID for customer

Back to top