KX-7000 Win7 64bit Universal Driver Release Note

2026-1-8

Support Platforms

Display Support

Change History

Installing and uninstalling driver

Support Platforms

Support CHIPS:

KX-7000 Chip

Support OS:

Win7 x64

Driver Version:

10.18.23.00-44.00.00

Back to top

Display Support

Support Device:

No. | Display Interface
1 | CRT/DP3/HDMI3/eDP3
2 | DP1/HDMI1/eDP1
3 | DP2/HDMI2/eDP2

HDMI/DP 支持的最大分辨率刷新率为 4096x2160@60Hz，CRT 支持的最大分辨率刷新率为 1920x1080@60Hz. 分辨率或者刷新率超出最大范围，需要提供显示器或者 panel 详细信息进一步评估。

Open API Support

1. OGL 4.6

2. OCL 1.2

DirectX API Support

1. DX 9.3

2. DX 10.1

3. DX 11.1

Video Codec Support

1. Decoding Capabilities

Format | Performance | Profile
H.265 HEVC | 1920x1080p60@100Mbps 3840x2160p60@60Mbps | MP
H.264 AVC | 1920x1080p60@90Mbps 3840x2160p30@90Mbps 3840x2160p60@12Mbps | HP
MPEG2 | 1920x1080p60@100Mbps 3840x2160p30@100M bps | MP@HL
MPEG4 | 1920x1080p30@30Mbps | ASP
M-JPEG | 1920x1080p30@130Mbps (M-JPEG) Baseline 8kx4k, 130Mpps (JPEG) | Baseline

Note:

We test this driver with VBIOS 38.F5.00.10, GOP V11.

Back to top

Change History

10.18.23.00-44.00.00(1/8/2026)

Initial Release for KX-7000.

Back to top

Installing and uninstalling driver

1 Installation

1) Installing the software by exe file

2) Run the installation program: setup.exe.

3) Choose the “next” button to install all the components of this package.

4) Once the installation finish, reboot system to complete the setup.

2 Uninstallation

1) Open ‘Control Panel’ and click ‘Uninstall a program’.

2) Find “ZX GPU Display Driver” and click Uninstall.

3) Choose the “Next” button to uninstall all the components of this package

4) Once the uninstallation finish, reboot system.

Back to top